#GEFID = 1, 0, 0
#COLUMNTEXT= 1
#COLUMNSEPARATOR= ;
#RECORDSEPARATOR= !
#FILEOWNER = Veldapps
#COMPANYID = Koops Grondmechanica, -, 31
#FILEDATE = 2019,11,26
#PROJECTID = GOVA 7a - Oeverwerken WHK, ZWV en KWN, 2018-1479, -
#COLUMN= 2
#COLUMNINFO= 1, m, bovenkant, 1
#COLUMNINFO= 2, m, onderkant, 2
#LASTSCAN= 10
#REPORTCODE = GEF-BORE-Report, 1, 0, 0, -
#MEASUREMENTCODE = NEN5104, 1, 0, 0, Normblad
#TESTID= WHK17.6
#ZID= 31000, 6.468, -
#MEASUREMENTTEXT= 9, maaiveld, vast horizontaal niveau
#XYID= 31000, 118987.752, 404825.154, -, -
#MEASUREMENTTEXT = 3, -, plaats boring
#MEASUREMENTTEXT = 16, 2019-7-9, datum boring
#MEASUREMENTTEXT = 13, Koops Grondmechanica, boorfirma
#MEASUREMENTVAR = 31, 0.1, m, diepte onderkant boortraject
#MEASUREMENTTEXT = 31, EDM, boormethode (edelman)
#MEASUREMENTVAR = 33, 0.9, m, diepte onderkant boortraject
#MEASUREMENTTEXT = 32, EDM, boormethode (edelman)
#MEASUREMENTVAR = 35, 1.3, m, diepte onderkant boortraject
#MEASUREMENTTEXT = 33, EDM, boormethode (edelman)
#MEASUREMENTVAR = 37, 1.5, m, diepte onderkant boortraject
#MEASUREMENTTEXT = 34, EDM, boormethode (edelman)
#MEASUREMENTVAR = 39, 2.0, m, diepte onderkant boortraject
#MEASUREMENTTEXT = 35, EDM, boormethode (edelman)
#MEASUREMENTVAR = 41, 4.0, m, diepte onderkant boortraject
#MEASUREMENTTEXT = 36, PUL, boormethode (pulsboor)
#MEASUREMENTVAR = 43, 6.5, m, diepte onderkant boortraject
#MEASUREMENTTEXT = 37, PUL, boormethode (pulsboor)
#MEASUREMENTVAR = 45, 6.8, m, diepte onderkant boortraject
#MEASUREMENTTEXT = 38, PUL, boormethode (pulsboor)
#MEASUREMENTVAR = 47, 7.8, m, diepte onderkant boortraject
#MEASUREMENTTEXT = 39, PUL, boormethode (pulsboor)
#MEASUREMENTVAR = 49, 10.0, m, diepte onderkant boortraject
#MEASUREMENTTEXT = 40, PUL, boormethode (pulsboor)
#MEASUREMENTTEXT = 5, 2019-7-9, datum boorbeschrijving
#MEASUREMENTTEXT = 6, John Loonstra, beschrijver lagen
#MEASUREMENTTEXT = 19, 2019-7-23, einddatum boring
#MEASUREMENTVAR = 16, 10.0, m, einddiepte
#MEASUREMENTTEXT = 23, John Loonstra, naam boormeester
#SPECIMENVAR = 1, 2, -, aantal monsters
#SPECIMENTEXT = 11, 1, monstercode monster 1
#SPECIMENVAR = 11, 6.9, m, bovenkant monster 1
#SPECIMENVAR = 12, 7.3, m, onderkant monster 1
#SPECIMENTEXT = 12, 2019-7-23, datum monster 1
#SPECIMENTEXT = 13, 10:15, tijd monster 1
#SPECIMENTEXT = 14, O, (on)geroerd monster 1
#SPECIMENTEXT = 18, 2, monstercode monster 2
#SPECIMENVAR = 18, 9.0, m, bovenkant monster 2
#SPECIMENVAR = 19, 10.0, m, onderkant monster 2
#SPECIMENTEXT = 19, 2019-7-23, datum monster 2
#SPECIMENTEXT = 20, 10:15, tijd monster 2
#SPECIMENTEXT = 21, G, (on)geroerd monster 2
#MEASUREMENTTEXT = 18, Nee, peilbuis afwezig
#MEASUREMENTVAR = 19, 0, -, aantal peilbuizen
#MEASUREMENTVAR = 18, 1.4, m, grondwaterstand direct na boring
#EOH=
0.0;0.1;'Zs2';'ZZF';'GR BR'!
0.1;0.9;'Zs2';'ZMF';'GE GR'!
0.9;1.3;'Zs2';'ZMF';'ZW BR'!
1.3;1.5;'Zs2';'ZZF';'GE BR'!
1.5;2.0;'Zs2';'ZZF';'GE BR'!
2.0;4.0;'Zs2';'ZMF';'GE BR'!
4.0;6.5;'Zs2';'ZMG';'GE BR'!
6.5;6.8;'Zs3';'ZMF';'GR'!
6.8;7.8;'Ks3';'GR'!
7.8;10.0;'Zs2';'ZMF';'GR'!