

Annex 2: Reference contracts 
	Project:
	European tender Geophysical Survey at the IJmuiden Ver Wind Farm Sites V and VI (IJ56)

	Company (Tenderer):
	



The contracting authority has set the following key competences that correspond to experience in essential aspects of the contract:
1. Provision of vessels and equipment, executing geophysical soil investigations, processing and comprehensive reporting for an offshore geophysical soil investigation in order to obtain high resolution geophysical information to 100 m depth that is suitable for development, engineering and installation purposes for an offshore wind farm involving the acquisition of; 
· High resolution bathymetry data using a Multi-Beam Echo Sounder (MBES), and;
· High resolution Side Scan Sonar and Magnetometer data, and;
· High-resolution seismic data using sub-bottom profilers, single-channel boomer or sparker acquisition, and ultra-high resolution multi-channel sparker or air gun sources of power suitable for the depth of interest, and;
· [bookmark: _Hlk85459931]Sampling of Seabed Sediments (ground truthing/environmental).
· Sampling of Sub-Seabed Sediments (Vibrocore sampling)
1. Execution of an investigation in which expert knowledge of the upper 100 m of the North Sea basin (seabed morphology, geology) was needed;
1. Provision of vessel and equipment for the execution of 3D UHRS site investigations. 


	Key competence 
For each competence fill in:
□ Key competence number (1, 2, 3 or combination)
□ Description of reference assignment (activities performed, results delivered)
□ Value of assignment in EUR
□ Commencement and end date of contract
□ Contact data of referee: company name, contact person, telephone/email
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Tenderer declares that he has carried out at least one reference assignment for each of the core competences listed above that meets the following minimum requirements:
· The subject of the reference assignment must be comparable to the core competence in question.
· The reference assignment must have been executed or completed within the three years prior to the closing date for the submission of tenders. If the Tenderer uses an assignment that is not yet fully complete, then only the completed results of the ongoing assignment can be submitted for reference purposes: projected results cannot be taken into consideration.
· The size of each investigated area, that is part of the object of reference, is at least 100 km2 (with exception of item 3, 3D UHRS survey) 

The total value of the reference assignment(s) must be at least EUR 1,500,000.

This reference-assignment value must exclusively consist of the value of the aspects of the assignment that are equivalent to the services specified in this document. In case a series of separate yet significantly comparable assignments was carried out for the same client during the reference period, then the turnover of these separate assignments can be combined into a cumulative total.

Assignments including one or more subcontractors can only be used as reference assignments if  the subcontractor(s) in question will be involved in the fulfilment of the Contract and if the Tenderer can and will make use of the knowledge and experience of the subcontractor(s) in question during the fulfilment of the assignment.


