<!DOCTYPE qgis PUBLIC 'http://mrcc.com/qgis.dtd' 'SYSTEM'>
<qgis version="3.30.0-'s-Hertogenbosch">
  <identifier></identifier>
  <parentidentifier></parentidentifier>
  <language></language>
  <type></type>
  <title></title>
  <abstract></abstract>
  <contact>
    <name></name>
    <organization></organization>
    <position></position>
    <voice></voice>
    <fax></fax>
    <email></email>
    <role></role>
  </contact>
  <links/>
  <dates/>
  <fees></fees>
  <encoding></encoding>
  <crs>
    <spatialrefsys nativeFormat="Wkt">
      <wkt>PROJCRS["Amersfoort / RD New",BASEGEOGCRS["Amersfoort",DATUM["Amersfoort",ELLIPSOID["Bessel 1841",6377397.155,299.1528128,LENGTHUNIT["metre",1]]],PRIMEM["Greenwich",0,ANGLEUNIT["degree",0.0174532925199433]],ID["EPSG",4289]],CONVERSION["RD New",METHOD["Oblique Stereographic",ID["EPSG",9809]],PARAMETER["Latitude of natural origin",52.1561605555556,ANGLEUNIT["degree",0.0174532925199433],ID["EPSG",8801]],PARAMETER["Longitude of natural origin",5.38763888888889,ANGLEUNIT["degree",0.0174532925199433],ID["EPSG",8802]],PARAMETER["Scale factor at natural origin",0.9999079,SCALEUNIT["unity",1],ID["EPSG",8805]],PARAMETER["False easting",155000,LENGTHUNIT["metre",1],ID["EPSG",8806]],PARAMETER["False northing",463000,LENGTHUNIT["metre",1],ID["EPSG",8807]]],CS[Cartesian,2],AXIS["easting (X)",east,ORDER[1],LENGTHUNIT["metre",1]],AXIS["northing (Y)",north,ORDER[2],LENGTHUNIT["metre",1]],USAGE[SCOPE["Engineering survey, topographic mapping."],AREA["Netherlands - onshore, including Waddenzee, Dutch Wadden Islands and 12-mile offshore coastal zone."],BBOX[50.75,3.2,53.7,7.22]],ID["EPSG",28992]]</wkt>
      <proj4>+proj=sterea +lat_0=52.1561605555556 +lon_0=5.38763888888889 +k=0.9999079 +x_0=155000 +y_0=463000 +ellps=bessel +units=m +no_defs</proj4>
      <srsid>2517</srsid>
      <srid>28992</srid>
      <authid>EPSG:28992</authid>
      <description>Amersfoort / RD New</description>
      <projectionacronym>sterea</projectionacronym>
      <ellipsoidacronym>EPSG:7004</ellipsoidacronym>
      <geographicflag>false</geographicflag>
    </spatialrefsys>
  </crs>
  <extent>
    <spatial maxx="0" minx="0" maxy="0" dimensions="2" minz="0" maxz="0" crs="" miny="0"/>
    <temporal>
      <period>
        <start></start>
        <end></end>
      </period>
    </temporal>
  </extent>
</qgis>
