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Annex 2b:  List of Reference contracts – LOT 2
	Project:
	Geotechnical Survey for: Doordewind Investigation area. 

	Tenderer:
	



[bookmark: _Hlk158736630]This Annex [2b] refers to requirements set-out in the Tender document, section 4.3.2 Reference data (technical qualifications). 

[bookmark: _Hlk158735654]The Tenderer is requested to provide details of reference projects of similar size and complexity (minimum 1, maximum 8) in this Annex. 
[bookmark: _Hlk157760785]Only references for projects completed in 2019 or later shall be considered. If the Tenderer uses an assignment that is not yet fully complete, then only the completed results of the ongoing assignment can be submitted for reference purposes. Projected results should not be provided and will not be taken into consideration. 

For each of the key experience requirements, at least one of the provided references shall fulfil the respective requirement. Minimum requirements in relation to investigation size (number of locations), target depth and contract values are summarized in the table below. If a provided reference reflects more than one key experience the Tenderer can use this same reference for multiple key competences.

The reference values must exclusively consist of the value of the aspects of the assignment that are equivalent to the service specified in this document. In case a series of separate, yet significantly comparable assignments, were carried out for the same client during the reference period, then the turnover of these separate assignments can be combined into a cumulative total.

The use of experience of one or more subcontractors in the references is only allowed if the subcontractors is involved in the execution of the WORKS described in this tender and as such the knowledge and experience of relevant subcontractor are at Tenderers disposal during the execution of the contract[footnoteRef:1]. [1:  Please be reminded that in the event that Tenderer wishes to include one or more reference contracts by a subcontractor, the subcontractor also needs to complete an ESPD form. For further instructions, reference is made to the Tender document, Section 7.3.17 Submission of a Tender in collaboration with other organizations] 


The contracting authority reserves the right to verify, if necessary, references for accuracy and completeness and to contact one or more references without intervention and/or permission from the tenderer. 


Key experience requirements
In Table 1 below 8 key experience requirements are listed. In Table 2 on the next page Tenderer is requested to provide details about the reference contracts (minimum 1, maximum 8). In Table 1 Tenderer shall check/ tick/ mark the appropriate box to indicate which reference fulfills which requirement


[bookmark: _Ref161686080]Table 1 - Key experience requirements for Lot 2
	[bookmark: _Hlk161677036]KEY EXPERIENCE, GENERAL
	A
	B
	C
	D
	E
	F
	G
	H

	1. [bookmark: _Hlk158736308]The execution of an offshore geotechnical survey (borehole campaign) to obtain geotechnical information that is suitable for development, engineering and installation purposes for an offshore wind farm (Minimum contract value EUR 2,500,000), including 
· Provision of vessels and geotechnical equipment;
· Data processing, laboratory testing and reporting.
	☐	☐	☐	☐	☐	☐	☐	☐
	2. Execution of a geotechnical survey in the North Sea, or similar geological conditions (soil conditions shall be predominantly non-cohesive); Minimum contract value EUR 1,000,000.
	☐	☐	☐	☐	☐	☐	☐	☐
	KEY EXPERIENCE, BOREHOLE SCOPE
	A
	B
	C
	D
	E
	F
	G
	H

	3. [bookmark: _Hlk158736375]Combined downhole sampling/PCPT boreholes, minimum 25 locations, with target depth ≥ 40m below seabed.
	☐	☐	☐	☐	☐	☐	☐	☐
	4. Downhole SCPT: minimum 10 locations with target depth ≥ 40m below seabed.
	☐	☐	☐	☐	☐	☐	☐	☐
	5. Downhole testing, PS-logging, minimum 50 tests, with target depth ≥ 40m below seabed. 
	☐	☐	☐	☐	☐	☐	☐	☐
	6. Downhole Geophysical Logging, density / porosity logging, minimum 25 tests, with target depth ≥ 40m below seabed).
	☐	☐	☐	☐	☐	☐	☐	☐
	KEY EXPERIENCE, LABORATORY TESTING SCOPE
	A
	B
	C
	D
	E
	F
	G
	H

	7. [bookmark: _Hlk158736521]Standard laboratory testing program, including Thermal Conductivity, Age Dating and MIC; Minimum contract value EUR 200,000.
	☐	☐	☐	☐	☐	☐	☐	☐
	8. Advanced laboratory testing program, including dynamic/ cyclic strength/ stiffness testing and drained cyclic triaxial testing; Minimum contract value EUR 50,000.
	☐	☐	☐	☐	☐	☐	☐	☐




Details of references
TENDERER to complete the table below (minimum 1, maximum 8 reference contracts). Under notes, TENDERER has the possibility to provide a short description of the project, for what type of development the survey was executed, and/ or provide details about the contracting entity if this was a company that TENDERER proposes as a subcontractor. 
[bookmark: _Ref161686084]Table 2 - List of reference contracts – Lot 2
	 REFERENCE A

	Project Name
	

	Client Name
	

	Location (country, sea)
	

	Year of completion
	
	Total contract value
	EUR 

	Provision of vessel and geotechnical spread
	YES / NO
	Vessel(s) (name, IMO)
	

	Contractor contracting entity
	

	Client contact referee (name, telephone, email)
	

	Notes:

	REFERENCE B

	Project Name
	

	Client Name
	

	Location (country, sea)
	

	Year of completion
	
	Total contract value
	EUR 

	Provision of vessel and geotechnical spread
	YES / NO
	Vessel(s) (name, IMO)
	

	Contractor contracting entity
	

	Client contact referee (name, telephone, email)
	

	Notes:

	[bookmark: _Hlk159575217]REFERENCE C

	Project Name
	

	Client Name
	

	Location (country, sea)
	

	Year of completion
	
	Total contract value
	EUR 

	Provision of vessel and geotechnical spread
	YES / NO
	Vessel(s) (name, IMO)
	

	Contractor contracting entity
	

	Client contact referee (name, telephone, email)
	

	Notes:

	REFERENCE D

	Project Name
	

	Client Name
	

	Location (country, sea)
	

	Year of completion
	
	Total contract value
	EUR 

	Provision of vessel and geotechnical spread
	YES / NO
	Vessel(s) (name, IMO)
	

	Contractor contracting entity
	

	Client contact referee (name, telephone, email)
	

	Notes:

	REFERENCE E

	Project Name
	

	Client Name
	

	Location (country, sea)
	

	Year of completion
	
	Total contract value
	EUR 

	Provision of vessel and geotechnical spread
	YES / NO
	Vessel(s) (name, IMO)
	

	Contractor contracting entity
	

	Client contact referee (name, telephone, email)
	

	Notes:

	REFERENCE F

	Project Name
	

	Client Name
	

	Location (country, sea)
	

	Year of completion
	
	Total contract value
	EUR 

	Provision of vessel and geotechnical spread
	YES / NO
	Vessel(s) (name, IMO)
	

	Contractor contracting entity
	

	Client contact referee (name, telephone, email)
	

	Notes:

	REFERENCE G

	Project Name
	

	Client Name
	

	Location (country, sea)
	

	Year of completion
	
	Total contract value
	EUR 

	Provision of vessel and geotechnical spread
	YES / NO
	Vessel(s) (name, IMO)
	

	Contractor contracting entity
	

	Client contact referee (name, telephone, email)
	

	Notes:

	REFERENCE H

	Project Name
	

	Client Name
	

	Location (country, sea)
	

	Year of completion
	
	Total contract value
	EUR 

	Provision of vessel and geotechnical spread
	YES / NO
	Vessel(s) (name, IMO)
	

	Contractor contracting entity
	

	Client contact referee (name, telephone, email)
	

	Notes:
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