Bijlage X – Aanvullende eisen motortest
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2.1 Test Protocols
Specification Machine Oosterpolder Pump 1 DAC Rev.2 Version 3.1.xIsx

Mandatory [Mandatory [IEC-34-1 [Test Sequence
TestsTM__|Tests PM
3.1 Visual Inspection x x R 1
3.2 Basic Tests x x R 2
33 Insulation resistance (cold) x x R 3
3.4 Winding resistance method (cold) X x R 4
ES Resistance measurement PT-100 (cold) X x R 5
3.6 Resistance PTC stop (cold) x x R 5
37 Resistance PTC warning (cold) X x R 7
38 Insulation AC High Potential Test (AC HiPot) X x R s
ES BEMF measurement (cold) - x - 9 only in case of PM machine
310 [Overspeed test X x R 10
311 [Temperature Rise Test ETD (cold & hot) X x R fm
312 [Temperature Rise Test Bearings (cold & hot) X x R 12
312 [Winding resistance method (hot) X x R 1
314 [Calculated winding temperature rise test X x R 1
315 [Load test x x R 15
316 [No-load test x x R 16
317 |Vibration test x x R v
318 [Noise test x x R 0
319 [Locked rotor test X - R 9 only in case of IM machine
320 |BEMF measurement (hot) - X - 20 only in case of PM machine
321 [Insulation tests (hot) X x R 21
322 |Resistance measurement PT-100 (hot) X x R 2

(a) Mandatory Tests to perform are depending on machine type: IM = Induction Machine, PM = Permanent Magnet Machine.
(b) X = Mandatory test that has been carried out, depents on IM or PM.
(c) IEC-34, refers to the comparable tests according to norm NEN EN IEC 60034-1, R = Routine Test, T=Type Test, - = not specified.





