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	Project:
	Geotechnical Survey for: 	IA IJmuiden Ver Wind Farm Zone 
	IA Nederwiek Wind Farm Zone 
	IA Hollandse Kust (west) Wind Farm Zone 


	Company:
	



	Key competency (1, 2, 3, 4, 5, 6, 7 or combination)
	Reference contract
	Commencement date of contract
	Reference contract value (€)

	Size of investigation area (km2)
	Contact referee
(telephone / email)

	

	
	
	
	
	

	

	
	
	
	
	

	

	
	
	
	
	

	

	
	
	
	
	

	

	
	
	
	
	

	

	
	
	
	
	



The contracting authority has set the following key competencies that correspond to experience in essential aspects of the contract:
1. Provision of vessels and equipment, executing of survey works, processing and reporting for an offshore geotechnical survey to obtain geotechnical information that is suitable for development, engineering and installation purposes for an offshore wind farm.
2. Execution of a survey in which expert knowledge of the geology in the southern North Sea, or similar geological conditions, was needed;
3. Carrying out combined downhole sampling/PCPT boreholes with a target depth between 60m and 80m;
4. Carrying out downhole seismic cone penetration testing (SCPT) to a target depth of up to 60m;
5. Carrying out downhole in-situ testing (PS-logging, density logging, spectral gamma logging, downhole magnetic resonance logging) to a target depth of up to 60m bsf;
6. Performance of standard and advanced laboratory soil testing, including dynamic/cyclic strength/stiffness testing, thermal conductivity testing, Age Dating and MIC testing laboratory testing programmes on large wind farms projects; and
7. Contractor shall prove familiarity with advanced testing by reference to project work previously undertaken and provide evidence of such, including drained cyclic triaxial testing.

For each key competency, present a reference that fulfils the requirements set out above. 

If more than one key competency fulfilling the set requirements is reflected in a single reference, then you can use the same reference for those key competencies. The contracting authority reserves the right to verify, if necessary, references for accuracy and completeness and to contact one or more references without intervention and/or permission from the tenderer.

Minimum requirements:
· The subject of the reference assignment must be comparable to the core competence in question.
· The reference assignment must have been executed or completed within the four years prior to the closing date for the submission of tenders. If the Tenderer uses an assignment that is not yet fully complete, then only the completed results of the ongoing assignment can be submitted for reference purposes: projected results cannot be taken into consideration.
· The size of each investigated area, that is part of the object of reference, is at least 100 km2.
· The reference assignment(s) must have for each individual core competence a minimum value of:
· [bookmark: _Hlk49339428]€ 1,000,000 for core competences 1, 2, 3, 4, and 5;
· € 200,000 	for core competences 6 and 7.

The use of experience of one or more subcontractors in the references is only allowed if this subcontractor is / these subcontractors are engaged during the execution of this agreement and the tenderer can actually have the knowledge and experience of the relevant subcontractor(s) at his disposal and will actually use this during the execution of the contract.
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