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This Annex 7 describe the Wishes for this Tender. For Wishes 1 to 7 tenderer has to show if the offered system meets the requested Wish. Yes or No.
Wishes 8 and 9 will be judged based on the comment given for these two wishes by Tenderer. 

	
	
Wish
	
Comment


	1.
	See for this wish number 6.3.13 in Chapter 6 of this Request for Proposal:

The system has a four (4) year preventive maintenance contract following the warranty period.

If the system will be offered with a 4-year preventive maintenance contract, ten points will be given for this wish. If not, no points shall be given to this wish (Yes or No).

	Yes or No ?

Answer: 

	2.
	See for this wish number 6.4.30 in Chapter 6 of this Request for Proposal:

The incubator should be able to offer the option to create hypoxia conditions.

If the system that is offered is able to have the option to create hypoxia conditions, five points will be given for this wish. If not, no points shall be given to this wish (Yes or No).

	Yes or No ?

Answer:

	3.
	See for this wish number 6.5.36 in Chapter 6 of this Request for Proposal:

The system features automated recognition of optical components.

If the system that is offered can automatically recognize optical components, five points will be given for this wish. If not, no points shall be given for this wish (Yes or No).

	Yes or No ?

Answer:

	4.
	 See for this wish number 6.6.39 in Chapter 6 of this Request for Proposal:

The system can be upgraded to provide spatially-resolved molecular dynamics in a single measurement

If the system that is offered can be upgraded to provide spatially-resolved molecular dynamics in a single measurement, ten points will be given for this wish. If not, no points shall be given for this wish (Yes or No).

	Yes or No ?

Answer:

	5.
	See for this wish number 6.6.40 in Chapter 6 of this Request for Proposal:

The system can be upgraded to measure flow velocity and direction (live / microfluidics).

If the system that is offered can be upgraded to measure flow velocity and direction (live/microfluidics), five points will be given for this wish. If not, no points shall be given for this wish (Yes or No).

	Yes or No? 

Answer:

	6.
	See for this wish number 6.6.41 in Chapter 6 of this Request for Proposal:

The system can be upgraded to perform instant volumetric imaging.

If the system that is offered can be upgraded to perform instant volumetric imaging, ten points will be given for this wish. If not, no points shall be given for this wish (Yes or No).

	Yes or No?

Answer:

	7.
	See for this wish number 6.6.42 in Chapter 6 of this Request for Proposal:

The system can be upgraded with a highly sensitive (High QE: >40%) spectral detector

If the system that is offered can be upgraded with a highly sensitive (High QE: >40%) spectral detector, five points will be given for this wish. If not, no points shall be given for this wish (Yes or No).

	Yes or No?

Answer:

	8.
	See for this wish number 6.6.43 in Chapter 6 of this Request for Proposal:

The system can be upgraded to include a software-based super-resolution option. This should be obtained by optimizing acquisition sampling and online processing with a special confocal deconvolution package. The maximum resolution desired must be close to 120 nm, lateral resolution.

This wish will be judged based on the maximum resolution that will be offered. 
	Answer: (Maximum of five points for this wish)

	9. 
	See for this wish number 6.7.44 in Chapter 6 of this Request for Proposal:

Collaboration between supplier and TU/e to implement the imaging workflow in the ERC Advanced Grant project ‘Intrap’ at the Microfab/lab at TU/e.

This wish will be judged based on your description of a suggested mode of collaboration, and on your proposed concrete potential contributions in the collaboration.

	Answer: (Maximum of  five points for this wish)
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